{
"polo17_suspension_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Independent Front Suspension",
        "value":600,
    },
    "slotType" : "polo17_suspension_F",
    "slots": [
        ["type", "default", "description"]
        ["polo17_brake_F","polo17_brake_F", "Front Brakes"],
        //The case() is for backwards compatibility for old configs that use "trackwidth_F" variable.
        //To change the base track width, edit the trackoffset_F offset in the expression.
        ["wheel_F_5","steelwheel_01a_15x7_F", "Front Wheels", {"nodeOffset":{"x":"$=case($trackwidth_F == nil, $trackoffset_F+0.250, $trackwidth_F)", "y":-1.29, "z":0.27}}],
        ["polo17_wheeldata_F","polo17_wheeldata_F", "Front Spindles", {"coreSlot":true}],
        ["polo17_strut_F","polo17_strut_F", "Front Struts"],
        ["polo17_swaybar_F","polo17_swaybar_F", "Front Sway Bar"],
        ["polo17_steering","polo17_steering", "Steering"],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$camber_FR", "range", "", "Wheel Alignment", 0.999, 0.95, 1.03, "Camber Adjust", "Adjusts the wheel camber angle", {"subCategory":"Front"}]
        ["$caster_FR", "range", "", "Wheel Alignment", 1, 0.98, 1.02, "Caster Adjust", "Adjusts forward rake of the steering axis", {"subCategory":"Front"}],
        ["$trackoffset_F", "range", "+m", "Wheels", 0.0, -0.02, 0.05, "Wheel Offset", "Spacing of the wheel from the hub", {"stepDis":0.001,"subCategory":"Front"}]
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_subframe_F", ["polo17_subframe_F"]],
        ["polo17_brace", ["polo17_subframe_F"]],
        ["polo17_lowerarm_F", ["polo17_lowermounts_a_F","polo17_lowermounts_b_F","polo17_lowerarm_F"]],
        ["polo17_hub_F", ["polo17_hub_F"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
          //--FRONT RUNNING GEAR--
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"collision":true},
         {"selfCollision":true},
         //strut suspension
         //lower
         {"group":"polo17_subframe_F"},
         {"nodeWeight":6.5},
         {"group":["polo17_lowermounts_a_F", "polo17_subframe_F"]},
         ["fx1r", -0.30, -1.36, 0.205, {"chemEnergy":200,"burnRate":0.3,"flashPoint":200,"specHeat":0.1,"smokePoint":150,"selfIgnitionCoef":false}],
         ["fx1l", 0.30, -1.36, 0.205, {"chemEnergy":200,"burnRate":0.3,"flashPoint":200,"specHeat":0.1,"smokePoint":150,"selfIgnitionCoef":false}],
         {"group":["polo17_lowermounts_b_F", "polo17_subframe_F"]},
         ["fx2r", -0.27, -0.97, 0.21],
         ["fx2l", 0.27, -0.97, 0.21],
         {"group":"polo17_subframe_F"},
         {"nodeWeight":2.6},
         ["fx3r", -0.025, -1.62, 0.20],
         ["fx3", 0.1, -1.65, 0.33, {"collision":false, "selfCollision":false}],
         ["fx3l", 0.2, -1.62, 0.20],
         ["fx4r", -0.27, -0.8, 0.21],
         ["fx4l", 0.27, -0.8, 0.21],
         ["fx6r", -0.4, -1.15, 0.4, {"nodeWeight":4.0}],
         ["fx6l", 0.4, -1.15, 0.4, {"nodeWeight":4.0}],
         ["fx7", 0.1, -1.9, 0.215, {"selfCollision":false}],

         //steering box/tie rod end
         {"nodeWeight":6.0},
         {"selfCollision":false},
         {"group":["polo17_steeringbox", "polo17_subframe_F"]},
         ["fx5r", -0.13, -1.13, 0.285],
         ["fx5l", 0.13, -1.13, 0.285],

         //--FRONT INDEPENDENT SUSPENSION--
         {"collision":true},
         {"selfCollision":true},
         //front hub
         {"nodeWeight":7.0},
         ["fh1r",-0.70, -1.33, 0.16, {"group":["polo17_lowerarm_F","polo17_hub_F","polo17_strut_F"]}],
         ["fh1l", 0.70, -1.33, 0.16, {"group":["polo17_lowerarm_F","polo17_hub_F","polo17_strut_F"]}],
         //tie rod end -- overwritten with drift steering
         {"nodeWeight":5.0},
         {"selfCollision":false},
         ["fh3r",-0.64, -1.165, 0.26, {"group":["polo17_tierod_F","polo17_hub_F"]}],
         ["fh3l", 0.64, -1.165, 0.26, {"group":["polo17_tierod_F","polo17_hub_F"]}],
         {"nodeWeight":4.5},
         ["fh4r",-0.593, -1.293, 0.606, {"group":["polo17_shockbottom_F","polo17_hub_F"]}],
         ["fh4l", 0.593, -1.293, 0.606, {"group":["polo17_shockbottom_F","polo17_hub_F"]}],
         {"selfCollision":true},
         ["fh5r",-0.72, -1.48, 0.295, {"group":["polo17_caliper_F","polo17_hub_F"]}],
         ["fh5l", 0.72, -1.48, 0.295, {"group":["polo17_caliper_F","polo17_hub_F"]}],
         {"nodeWeight":3.5},
         {"selfCollision":false},
         ["fw2r",-0.72, -1.14, 0.295, {"group":["polo17_wheelarm_F","polo17_hub_F"]}],
         ["fw2l", 0.72, -1.14, 0.295, {"group":["polo17_wheelarm_F","polo17_hub_F"]}],
         //strut flexbody node
         {"nodeWeight":0.25},
         {"group":["polo17_strut_F"]},
         {"collision":false},
         {"selfCollision":false},
         ["fs2l", 0.48, -1.28, 0.55],
         ["fs2r", -0.48, -1.28, 0.55],
         {"group":""},
    ],
    "rails": {
        "strut_FR":{"links:":["fh1r", "fs1r"], "broken:":[], "looped":false, "capped":true},
        "strut_FL":{"links:":["fh1l", "fs1l"], "broken:":[], "looped":false, "capped":true},
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fh4r", "strut_FR", true, true, 0.0, 18001000, "FLT_MAX", "FLT_MAX"],
        ["fh4l", "strut_FL", true, true, 0.0, 18001000, "FLT_MAX", "FLT_MAX"],
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        {"spring":180000, "damp":0, "deform":25000, "strength":100000},
        //rigidify steering arm
        ["fw1rr", "fw1r", "fh1r", "fh3r"],
        ["fw1ll", "fw1l", "fh1l", "fh3l"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--FRONT SUBFRAME--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":4001000,"beamDamp":180},
          {"beamDeform":25000,"beamStrength":"FLT_MAX"},
          {"deformLimitExpansion":1.1},
          //main shape center mount
          ["fx6r", "fx1r"],
          ["fx6r", "fx2r"],
          ["fx6l", "fx1l"],
          ["fx6l", "fx2l"],
          //main shape lengthwise
          //axis points
          ["fx1l", "fx2l"],
          ["fx1r", "fx2r"],
          //front mount
          {"beamDeform":9000},
          ["fx1r", "fx3r"],
          ["fx3r", "fx7"],
          ["fx1l", "fx3l"],
          ["fx3l", "fx7"],
          //rear mount
          {"beamDeform":15000},
          ["fx2l", "fx4l"],
          ["fx2r", "fx4r"],
          //main shape widthwise
          //axis points
          ["fx1l", "fx1r"],
          ["fx2l", "fx2r"],
          //front mount
          ["fx3l", "fx3r"],

          //crossing
          {"beamDeform":11000},
          {"deformLimitExpansion":""},
          //center mount
          ["fx6r", "fx1l"],
          ["fx6r", "fx2l"],
          ["fx6l", "fx1r"],
          ["fx6l", "fx2r"],
          //axis points
          {"beamDeform":16000,},
          ["fx1l", "fx2r"],
          ["fx2l", "fx1r"],
          //rear mount
          {"beamDeform":7000},
          ["fx4l", "fx2r"],
          ["fx4r", "fx2l"],
          //front mount
          {"beamDeform":4000},
          ["fx3l", "fx1r"],
          ["fx1l", "fx3r"],

          //rigids
          {"beamSpring":4001000,"beamDamp":180},
          {"beamDeform":5000},
          //lengthwise
          //["fx7", "fx1r"],
          //["fx7", "fx1l"],
          //["fx3r", "fx2r"],
          //["fx3l", "fx2l"],
          ["fx1r", "fx4r"],
          ["fx1l", "fx4l"],
          //corner
          {"beamDeform":8000},
          ["fx6r", "fx4r"],
          ["fx6l", "fx4l"],
          ["fx6r", "fx3r"],
          ["fx6l", "fx3l"],

          //rigidifier
          {"beamDeform":6000},
          {"beamSpring":401000,"beamDamp":180},
          ["fx3", "fx3r"],
          ["fx3", "fx3l"],
          ["fx3", "fx7"],
          ["fx3", "fx1r"],
          ["fx3", "fx1l"],
          ["fx3", "fx6r"],
          ["fx3", "fx6l"],

          //steering rack
          {"beamSpring":4501000,"beamDamp":180},
          {"beamDeform":25000},
          ["fx5r","fx5l"],
          ["fx5r","fx1r"],
          ["fx5l","fx1l"],
          ["fx5r","fx1l"],
          ["fx5l","fx1r"],
          ["fx5r","fx2l"],
          ["fx5l","fx2r"],
          ["fx5r","fx2r"],
          ["fx5l","fx2l"],

          //attach to body
          {"beamSpring":1501000,"beamDamp":180},
          {"beamDeform":9500,"beamStrength":70000},
          //front
          {"breakGroup":"subframemount_FF"},
          ["fx7", "f18l"],
          ["fx7", "f18r"],
          ["fx7", "f11ll"],
          ["fx7", "f11rr"],
          ["fx7", "f10ll"],
          ["fx7", "f10rr"],
          ["fx7", "f18"],
          //rear
          {"beamDeform":8000,"beamStrength":80000},
          {"breakGroup":"subframemount_FRR"},
          ["fx4r", "f1r"],
          ["fx4r", "f5r"],
          ["fx4r", "f1l"],
          ["fx4r", "f5l"],
          ["fx4r", "f2r"],
          {"breakGroup":"subframemount_FRL"},
          ["fx4l", "f1r"],
          ["fx4l", "f5r"],
          ["fx4l", "f1l"],
          ["fx4l", "f5l"],
          ["fx4l", "f2l"],
          //center
          {"beamSpring":4501000,"beamDamp":100},
          {"beamDeform":22000,"beamStrength":70000},
          {"breakGroup":"subframemount_FMR"},
          ["fx6r", "f5r"],
          ["fx6r", "f1r"],
          ["fx6r", "f5l"],
          ["fx6r", "f1l"],
          ["fx6r", "f12rr"],
          ["fx6r", "f10rr"],
          ["fx1r", "f12rr"],
          ["fx1r", "f5r"],
          {"breakGroup":"subframemount_FML"},
          ["fx6l", "f5l"],
          ["fx6l", "f1l"],
          ["fx6l", "f5r"],
          ["fx6l", "f1r"],
          ["fx6l", "f12ll"],
          ["fx6l", "f10ll"],
          ["fx1l", "f12ll"],
          ["fx1l", "f5l"],
          {"breakGroup":""},

          //limiter
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":2},
          {"beamSpring":4001000,"beamDamp":180},
          {"beamDeform":15000,"beamStrength":80000},
          {"deformLimitExpansion":""}
          ["fx2r", "f5r"],
          ["fx2l", "f5l"],
          ["fx7", "f15l"],
          ["fx7", "f15r"],
          {"beamPrecompression":0.7},
          ["fx1r", "f12rr"],
          ["fx1l", "f12ll"],

           //--FRONT INDEPENDENT SUSPENSION--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          //mcpherson strut suspension
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":8501000,"beamDamp":100},
          {"beamDeform":85000,"beamStrength":350000},
          {"deformLimitExpansion":1.1},
          //front hub
          ["fh1r","fh3r"],
          ["fh1l","fh3l"],
          ["fh3r","fh4r"],
          ["fh3l","fh4l"],
          ["fh1r","fh4r"],
          ["fh1l","fh4l"],
          ["fh1r","fh5r"],
          ["fh1l","fh5l"],
          ["fh3r","fh5r"],
          ["fh3l","fh5l"],
          ["fh4r","fh5r"],
          ["fh4l","fh5l"],

          {"beamSpring":6001000,"beamDamp":100},
          ["fw2r","fh1r"],
          ["fw2r","fh3r"],
          ["fw2r","fh4r"],
          ["fw2r","fh5r"],
          ["fw2l","fh1l"],
          ["fw2l","fh3l"],
          ["fw2l","fh4l"],
          ["fw2l","fh5l"],

          {"beamSpring":8501000,"beamDamp":100},
          {"beamDeform":85000,"beamStrength":275000},
          {"optional":true},
          //attach to wheel
          {"breakGroup":"wheel_FR"},
          ["fh1r","fw1r", {"name":"axle_FR"}],
          ["fh3r","fw1r", {"beamSpring":13001000,"beamDamp":20}],
          ["fh4r","fw1r"],
          ["fh5r","fw1r"],
          ["fw2r","fw1r", {"beamSpring":6001000,"beamDamp":20}],
          ["fh1r","fw1rr"],
          ["fh3r","fw1rr", {"beamSpring":13001000,"beamDamp":20}],
          ["fh5r","fw1rr"],
          ["fw2r","fw1rr", {"beamSpring":6001000,"beamDamp":20}],
          {"breakGroup":"wheel_FL"},
          ["fh1l","fw1l", {"name":"axle_FL"}],
          ["fh3l","fw1l", {"beamSpring":13001000,"beamDamp":20}],
          ["fh4l","fw1l"],
          ["fh5l","fw1l"],
          ["fw2l","fw1l", {"beamSpring":6001000,"beamDamp":20}],
          ["fh1l","fw1ll"],
          ["fh3l","fw1ll", {"beamSpring":13001000,"beamDamp":20}],
          ["fh5l","fw1ll"],
          ["fw2l","fw1ll", {"beamSpring":6001000,"beamDamp":20}],
          //camber
          {"breakGroup":"wheel_FR"},
          ["fh4r","fw1rr", {"beamPrecompression":"$camber_FR","beamPrecompressionTime":0.5}],
          {"breakGroup":"wheel_FL"},
          ["fh4l","fw1ll", {"beamPrecompression":"$camber_FR","beamPrecompressionTime":0.5}],
          {"breakGroup":""},
          {"optional":false},

          //strut flexbody node
         {"beamSpring":501000,"beamDamp":50,"beamDeform":37500,"beamStrength":"FLT_MAX"},
          ["fh4r","fs2r"],
          ["fh4l","fs2l"],
          ["fh3r","fs2r"],
          ["fh3l","fs2l"],
          ["fh5r","fs2r"],
          ["fh5l","fs2l"],

          //lower arm
          {"beamSpring":13001000,"beamDamp":2000},
          {"beamDeform":75000,"beamStrength":450000},
          ["fx2r","fh1r", {"beamPrecompression":"$caster_FR","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          ["fx2l","fh1l", {"beamPrecompression":"$caster_FR","beamPrecompressionTime":0.5,"dampCutoffHz":500}],
          ["fx1r","fh1r", {"dampCutoffHz":500}],
          ["fx1l","fh1l", {"dampCutoffHz":500}],

          //front limiters
          {"deformLimitExpansion":""},
          {"beamPrecompression":0.7, "beamType":"|SUPPORT", "beamLongBound":3},
          {"beamSpring":8001000,"beamDamp":1000,"beamDeform":165000,"beamStrength":900000},
          //firewall
          {"optional":true},
          //{"breakGroupType":1},
          //{"breakGroup":"wheel_FR"},
          ["fw1rr","f19rr"],
          ["fw1rr","f1rr"],
          ["fw1rr","f1r"],
          ["fw1rr","f5r"],
          ["fw1r","f1rr"],
          ["fw1r","f5r"],
          //{"breakGroup":"wheel_FL"},
          ["fw1ll","f19ll"],
          ["fw1ll","f1ll"],
          ["fw1ll","f1l"],
          ["fw1ll","f5l"],
          ["fw1l","f1ll"],
          ["fw1l","f5l"],
          //{"breakGroup":""},
          //{"breakGroupType":0},
          {"optional":false},

          {"beamPrecompression":0.73, "beamType":"|SUPPORT"},
          ["fh1r","f5r"],
          ["fh1l","f5l"],
          ["fh1r","f6r"],
          ["fh1l","f6l"],
          ["fh1r","f6rr"],
          ["fh1l","f6ll"],
          ["fh3r","f5r"],
          ["fh3l","f5l"],
          ["fh3r","f1r"],
          ["fh3l","f1l"],
          ["fh4r","f1r"],
          ["fh4l","f1l"],
          ["fh4r","f1rr"],
          ["fh4l","f1ll"],

          //steering limit
          {"beamPrecompression":1, "beamType":"|SUPPORT", "beamLongBound":3},
          {"beamSpring":2501000,"beamDamp":150,"beamDeform":100000,"beamStrength":"FLT_MAX"},
          {"beamPrecompression":0.63},
          ["fh3r","fx1r"],
          ["fh3l","fx1l"],
          {"beamPrecompression":0.63},
          ["fw2r","fx1r"],
          ["fw2l","fx1l"],
          {"beamPrecompression":0.85},
          ["fh5r","fx2r"],
          ["fh5l","fx2l"],
          {"beamPrecompression":1.0},

          //hard travel limit
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1, "beamShortBound":1},
          {"beamDeform":15000,"beamStrength":150000},
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":1001000,"beamLimitDamp":1000},
          ["fh1r","fs1r", {"longBoundRange":0.12,"shortBoundRange":0.09,"boundZone":0.025,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          ["fh1l","fs1l", {"longBoundRange":0.12,"shortBoundRange":0.09,"boundZone":0.025,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"deformLimitExpansion":1.1},
    ],
    "triangles": [
            ["id1:","id2:","id3:"],
            //suspension shape
            {"triangleType":"NONCOLLIDABLE"},
            ["fx2r", "fx1r", "fh1r"],
            ["fh1r", "fh5r", "fw2r"],
            ["fh4r", "fw2r", "fh5r"],
            ["fh3r", "fh1r", "fw2r"],

            ["fx1l", "fx2l", "fh1l"],
            ["fh5l", "fh1l", "fw2l"],
            ["fw2l", "fh4l", "fh5l"],
            ["fh1l", "fh3l", "fw2l"],
            {"triangleType":"NORMALTYPE"},
    ],
    "pressureWheels": [
            ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
            //cancel out brake properties
            {"brakeTorque":0},
            {"parkingTorque":0},
            {"enableBrakeThermals":false},
            {"brakeDiameter":false},
            {"brakeMass":false},
            {"brakeType":false},
            {"rotorMaterial":false},
            {"brakeVentingCoef":false},
    ],
},
"polo17_wheeldata_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Spindles",
        "value":100,
    }
    "slotType" : "polo17_wheeldata_F",
    "pressureWheels": [
        ["name","hubGroup","group","node1:","node2:","nodeS","nodeArm:","wheelDir"],
        //front
        {"selfCollision":false}
        {"collision":true}
        {"hubcapBreakGroup":"hubcap_FR"},
        {"hubcapGroup":"hubcap_FR"},
        {"axleBeams":["axle_FR"]},
        ["FR", "wheel_FR", "tire_FR", "fw1rr", "fw1r", 9999, "fh5r", 1, {"torqueCoupling:":"fh1r", "torqueArm:":"fh4r", "torqueArm2:":"fw1rr","steerAxisUp:":"fs1r","steerAxisDown:":"fh1r"}],
        {"hubcapBreakGroup":"hubcap_FL"},
        {"hubcapGroup":"hubcap_FL"},
        {"axleBeams":["axle_FL"]},
        ["FL", "wheel_FL", "tire_FL", "fw1ll", "fw1l", 9999, "fh5l", -1, {"torqueCoupling:":"fh1l", "torqueArm:":"fh4l", "torqueArm2:":"fw1ll","steerAxisUp:":"fs1l","steerAxisDown:":"fh1l"}],
        {"selfCollision":true}
        {"axleBeams":[]},{"disableMeshBreaking":false,"disableTriangleBreaking":false},
        {"hubcapBreakGroup":""},
        {"hubcapGroup":""},
        {"enableHubcaps":false},
        {"enableTireLbeams":false},
        {"enableTreadReinfBeams":false},
        {"enableTireReinfBeams":false},
        {"enableTreadReinfBeams":false},
        {"enableTirePeripheryReinfBeams":false},
        {"loadSensitivitySlope":""},
        {"noLoadCoef":""},
        {"fullLoadCoef":""},
        {"frictionCoef":""},
        {"slidingFrictionCoef":""},
        {"softnessCoef":0.5},
        {"treadCoef":1.0},
    ],
    "powertrain" : [
        ["type", "name", "inputName", "inputIndex"],
        ["shaft", "spindleFL", "wheelaxleFL", 1, {"connectedWheel":"FL", "breakTriggerBeam":"axle_FL", "uiName":"Front Left Axle", "friction":0.98, "dynamicFriction":0.0021}],
        ["shaft", "spindleFR", "wheelaxleFR", 1, {"connectedWheel":"FR", "breakTriggerBeam":"axle_FR", "uiName":"Front Right Axle", "friction":0.98, "dynamicFriction":0.0021}],
    ],
},

"polo17_strut_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Struts",
        "value":200,
    },
    "slotType" : "polo17_strut_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_F", ["polo17_shocktop_F","polo17_shockbottom_F","polo17_strut_F"]],
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs with soft initial bump stop
          {"beamPrecompression":1, "beamType":"|BOUNDED","beamLongBound":1,"beamShortBound":1},
          {"beamDeform":17000,"beamStrength":180000},
          {"beamSpring":27000,"beamDamp":0},
          {"beamLimitSpring":54000,"beamLimitDamp":1000},
          ["fh4r","fs1r", {"precompressionRange":0.112,"longBoundRange":1,"shortBoundRange":0.142,"boundZone":0.08,"beamLimitDampRebound":0,"dampCutoffHz":500,
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.3,"attackFactor":8,"volumeFactor":2.05,"decayFactor":12,"noiseFactor":0.00,"pitchFactor":0.2,"maxStress":1200}],
          ["fh4l","fs1l", {"precompressionRange":0.112,"longBoundRange":1,"shortBoundRange":0.142,"boundZone":0.08"beamLimitDampRebound":0,"dampCutoffHz":500,
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.3,"attackFactor":8,"volumeFactor":2.05,"decayFactor":12,"noiseFactor":0.00,"pitchFactor":0.2,"maxStress":1200}],
          //dampers
          {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDamp":3800},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          ["fh1r","fs1r", {"beamDampFast":1300,"beamDampRebound":6000,"beamDampReboundFast":3000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
          ["fh1l","fs1l", {"beamDampFast":1300,"beamDampRebound":6000,"beamDampReboundFast":3000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
          //harder bump stop
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":181000,"beamLimitDamp":10000},
          ["fh4r","fs1r", {"longBoundRange":0.08,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          ["fh4l","fs1l", {"longBoundRange":0.08,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
}
"polo17_strut_F_sport_S": {
    "information":{
        "authors":"BeamNG",
        "name":"Sport S Front Struts",
        "value":350,
    },
    "slotType" : "polo17_strut_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_F", ["polo17_shocktop_F","polo17_shockbottom_F","polo17_strut_F"]],
    ],
    "beams": [
         ["id1:", "id2:"],
         //front springs with soft initial bump stop
         {"beamPrecompression":1, "beamType":"|BOUNDED","beamLongBound":1,"beamShortBound":1},
         {"beamDeform":17000,"beamStrength":180000},
         {"beamSpring":35000,"beamDamp":0},
         {"beamLimitSpring":52500,"beamLimitDamp":1000},
         ["fh4r","fs1r", {"precompressionRange":0.075,"longBoundRange":1,"shortBoundRange":0.117,"boundZone":0.08,"beamLimitDampRebound":0,"dampCutoffHz":500,
             "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.5,"attackFactor":33,"volumeFactor":2.0,"decayFactor":30,"noiseFactor":0.00,"pitchFactor":0.3,"maxStress":1500}],
         ["fh4l","fs1l", {"precompressionRange":0.075,"longBoundRange":1,"shortBoundRange":0.117,"boundZone":0.08,"beamLimitDampRebound":0,"dampCutoffHz":500,
             "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.5,"attackFactor":33,"volumeFactor":2.0,"decayFactor":30,"noiseFactor":0.00,"pitchFactor":0.3,"maxStress":1500}],
         //dampers
         {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
         {"beamSpring":0,"beamDamp":4400},
         {"beamLimitSpring":0,"beamLimitDamp":0},
         ["fh1r","fs1r", {"beamDampFast":1500,"beamDampRebound":9000,"beamDampReboundFast":3000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
         ["fh1l","fs1l", {"beamDampFast":1500,"beamDampRebound":9000,"beamDampReboundFast":3000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
         //harder bump stop
         {"beamSpring":0,"beamDamp":0},
         {"beamLimitSpring":181000,"beamLimitDamp":10000},
         ["fh4r","fs1r", {"longBoundRange":0.08,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
         ["fh4l","fs1l", {"longBoundRange":0.08,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
         {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
}
"polo17_strut_F_sport_RS": {
    "information":{
        "authors":"BeamNG",
        "name":"Sport RS Front Struts",
        "value":600,
    },
    "slotType" : "polo17_strut_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_F", ["polo17_shocktop_F","polo17_shockbottom_F","polo17_strut_F"]],
    ],
    "beams": [
         ["id1:", "id2:"],
         //front springs with soft initial bump stop
         {"beamPrecompression":1, "beamType":"|BOUNDED","beamLongBound":1,"beamShortBound":1},
         {"beamDeform":17000,"beamStrength":180000},
         {"beamSpring":42000,"beamDamp":0},
         {"beamLimitSpring":63000,"beamLimitDamp":1000},
         ["fh4r","fs1r", {"precompressionRange":0.054,"longBoundRange":1,"shortBoundRange":0.098,"boundZone":0.08,"beamLimitDampRebound":0,"dampCutoffHz":500,
             "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.5,"attackFactor":36,"volumeFactor":2.05,"decayFactor":70,"noiseFactor":0.00,"pitchFactor":0.4,"maxStress":1500}],
         ["fh4l","fs1l", {"precompressionRange":0.054,"longBoundRange":1,"shortBoundRange":0.098,"boundZone":0.08,"beamLimitDampRebound":0,"dampCutoffHz":500,
             "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.5,"attackFactor":36,"volumeFactor":2.05,"decayFactor":70,"noiseFactor":0.00,"pitchFactor":0.4,"maxStress":1500}],
         //dampers
         {"beamPrecompression":1, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
         {"beamSpring":0,"beamDamp":4600},
         {"beamLimitSpring":0,"beamLimitDamp":0},
         ["fh1r","fs1r", {"beamDampFast":1600,"beamDampRebound":10000,"beamDampReboundFast":5000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
         ["fh1l","fs1l", {"beamDampFast":1600,"beamDampRebound":10000,"beamDampReboundFast":5000,"beamDampVelocitySplit":0.2,"dampCutoffHz":500}],
         //harder bump stop
         {"beamSpring":0,"beamDamp":0},
         {"beamLimitSpring":181000,"beamLimitDamp":10000},
         ["fh4r","fs1r", {"longBoundRange":0.07,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
         ["fh4l","fs1l", {"longBoundRange":0.07,"shortBoundRange":0.085,"boundZone":0.04,"beamLimitDampRebound":0,"dampCutoffHz":500}],
         {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_strut_F_race": {
    "information":{
        "authors":"BeamNG",

        "name":"Race Front Coilovers",
        "value":850,
    },
    "slotType" : "polo17_strut_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_F", ["polo17_shocktop_F","polo17_shockbottom_F","polo17_strut_F"]],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$springheight_F", "range", "+m", "Suspension", 0, -0.06, 0.04, "Spring Height", "Raise or lower the suspension height", {"stepDis":0.005, "subCategory":"Front"}]
        ["$spring_F", "range", "N/m", "Suspension", 81000, 20000, 120000, "Spring Rate", "Spring stiffness", {"stepDis":500, "subCategory":"Front"}]
        ["$damp_bump_F", "range", "N/m/s", "Suspension", 6500, 500, 12500, "Bump Damping", "Damper rate in compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_rebound_F", "range", "N/m/s", "Suspension", 17000, 500, 25000, "Rebound Damping", "Damper rate in extension", {"stepDis":100, "subCategory":"Front"}]
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs without soft bump stop
          {"beamType":"|NORMAL"},
          {"beamDeform":17000,"beamStrength":180000},
          {"beamSpring":"$spring_F","beamDamp":0},
          //IMPORTANT: if precompressionRange is ~= nil then it supersedes beamPrecompression.
          //The case() is for backwards compatibility for old configs containing the "rideheight_F" variable.
          //To change the base ride height, edit the springheight_F offset in the expression.
          ["fh4r","fs1r", {"beamPrecompression":"$=$rideheight_F", "precompressionRange":"$=case($rideheight_F == nil, $springheight_F + 0.015, '')",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":1.0,"attackFactor":60,"volumeFactor":1.8,"decayFactor":80,"noiseFactor":0.00,"pitchFactor":1.0,"maxStress":2000}],

          ["fh4l","fs1l", {"beamPrecompression":"$=$rideheight_F", "precompressionRange":"$=case($rideheight_F == nil, $springheight_F + 0.015, '')",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":1.0,"attackFactor":60,"volumeFactor":1.8,"decayFactor":80,"noiseFactor":0.00,"pitchFactor":1.0,"maxStress":2000}],

          //dampers
          {"beamPrecompression":1.0, "beamType":"|BOUNDED","beamLongBound":1.0,"beamShortBound":1.0},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamSpring":0,"beamDamp":"$damp_bump_F"},
          ["fh1r","fs1r", {"beamDampRebound":"$damp_rebound_F","beamDampVelocitySplit":0.3,"beamDampFast":"$=$damp_bump_F / 3","beamDampReboundFast":"$=$damp_rebound_F / 3","dampCutoffHz":500}],
          ["fh1l","fs1l", {"beamDampRebound":"$damp_rebound_F","beamDampVelocitySplit":0.3,"beamDampFast":"$=$damp_bump_F / 3","beamDampReboundFast":"$=$damp_rebound_F / 3","dampCutoffHz":500}],
          //bump and rebound stops
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":251000,"beamLimitDamp":2000},
          ["fh4r","fs1r", {"longBoundRange":0.03,"shortBoundRange":0.07,"boundZone":0.02,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          ["fh4l","fs1l", {"longBoundRange":0.03,"shortBoundRange":0.07,"boundZone":0.02,"beamLimitDampRebound":0,"dampCutoffHz":500}],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_strut_F_rally": {
    "information":{
        "authors":"BeamNG",
        "name":"Rally Front Coilovers",
        "value":900,
    },
    "slotType" : "polo17_strut_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_F", ["polo17_shocktop_F","polo17_strut_F","polo17_shockbottom_F"]],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$springheight_F", "range", "+m", "Suspension", 0, -0.04, 0.06, "Spring Height", "Raise or lower the suspension height", {"stepDis":0.005, "subCategory":"Front"}]
        ["$spring_F", "range", "N/m", "Suspension", 40000, 10000, 80000, "Spring Rate", "Spring stiffness", {"stepDis":500,"subCategory":"Front"}]
        ["$damp_bump_F", "range", "N/m/s", "Suspension", 4500, 500, 10000, "Bump Damping", "Damper rate in slow compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_bump_F_fast", "range", "N/m/s", "Suspension", 3400, 500, 10000, "Fast Bump Damping", "Damper rate in fast compression", {"stepDis":100, "subCategory":"Front"}]
        ["$damp_rebound_F", "range", "N/m/s", "Suspension", 6400, 500, 10000, "Rebound Damping", "Damper rate in extension", {"stepDis":100,"subCategory":"Front"}]
        ["$damp_rebound_F_fast", "range", "N/m/s", "Suspension", 2100, 500, 10000, "Fast Rebound Damping", "Damper rate in fast extension", {"stepDis":100,"subCategory":"Front"}]
    ],
    "beams": [
          ["id1:", "id2:"],
          //front springs without soft bump stop
          {"beamType":"|NORMAL"},
          {"beamDeform":22000,"beamStrength":240000},
          {"beamSpring":"$spring_F","beamDamp":0},
          //IMPORTANT: if precompressionRange is ~= nil then it supersedes beamPrecompression.
          //The case() is for backwards compatibility for old configs containing the "rideheight_F" variable.
          //To change the base ride height, edit the springheight_F offset in the expression.
          ["fh4r","fs1r", {"beamPrecompression":"$=$rideheight_F", "precompressionRange":"$=case($rideheight_F == nil, $springheight_F + 0.117, '')",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.7,"attackFactor":7,"volumeFactor":2.05,"decayFactor":9,"noiseFactor":0.00,"pitchFactor":0.7,"maxStress":2000}],
          ["fh4l","fs1l", {"beamPrecompression":"$=$rideheight_F", "precompressionRange":"$=case($rideheight_F == nil, $springheight_F + 0.117, '')",
              "soundFile":"event:>Vehicle>Suspension>car_modn_med_01>spring_compress_01","colorFactor":0.7,"attackFactor":7,"volumeFactor":2.05,"decayFactor":9,"noiseFactor":0.00,"pitchFactor":0.7,"maxStress":2000}],

          //dampers
          {"beamPrecompression":1.0, "beamType":"|BOUNDED","beamLongBound":1.0,"beamShortBound":1.0},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          //bump
          {"beamSpring":0,"beamDamp":"$damp_bump_F"},
          ["fh1r","fs1r", {"beamDampRebound":0,"beamDampVelocitySplit":0.3,"beamDampFast":"$damp_bump_F_fast","beamDampReboundFast":0,"dampCutoffHz":500}],
          ["fh1l","fs1l", {"beamDampRebound":0,"beamDampVelocitySplit":0.3,"beamDampFast":"$damp_bump_F_fast","beamDampReboundFast":0,"dampCutoffHz":500}],
          //rebound
          {"beamSpring":0,"beamDamp":0},
          ["fh1r","fs1r", {"beamDampRebound":"$damp_rebound_F","beamDampVelocitySplit":0.2,"beamDampFast":0,"beamDampReboundFast":"$damp_rebound_F_fast","dampCutoffHz":500}],
          ["fh1l","fs1l", {"beamDampRebound":"$damp_rebound_F","beamDampVelocitySplit":0.2,"beamDampFast":0,"beamDampReboundFast":"$damp_rebound_F_fast","dampCutoffHz":500}],
          //hydraulic bump stop
          {"beamSpring":0,"beamDamp":0},
          {"beamLimitSpring":10000,"beamLimitDamp":15000},
          ["fh4r","fs1r", {"longBoundRange":1,"shortBoundRange":0.035,"boundZone":0.01,"beamLimitDampRebound":1000,"dampCutoffHz":250}],
          ["fh4l","fs1l", {"longBoundRange":1,"shortBoundRange":0.035,"boundZone":0.01,"beamLimitDampRebound":1000,"dampCutoffHz":250}],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_swaybar_F": {
    "information":{
        "authors":"BeamNG",
        "name":"Front Sway Bar",
        "value":110,
    },
    "slotType" : "polo17_swaybar_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_swaybar_F", ["polo17_lowermounts_a_F","polo17_lowermounts_b_F","polo17_shockbottom_F","polo17_lowerarm_F"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //anti-roll
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":""},
         {"selfCollision":false},
         {"collision":true}
         {"nodeWeight":1.5},
         //front anti-roll
         ["arbfr", -0.58, -1.31, 0.25],
         ["arbfl", 0.58, -1.31, 0.25],
         {"group":""},
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        //19mm 1403
        //20mm 1722
        //21mm 2094
        //22mm 2522
        //23mm 3012
        {"spring":1722, "damp":10, "deform":10000, "strength":9999999},
        ["arbfr", "fx2r", "fx2l", "arbfl"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--ANTI-ROLL--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":2501000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":250000},
          //end links
          ["arbfr","fh4r"],
          ["arbfl","fh4l"],
          //rigids
          ["arbfr","fx2r"],
          ["arbfl","fx2l"],
          ["arbfr","fx2l"],
          ["arbfl","fx2r"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_swaybar_F_sport": {
    "information":{
        "authors":"BeamNG",
        "name":"Sport Front Sway Bar",
        "value":200,
    },
    "slotType" : "polo17_swaybar_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_swaybar_F", ["polo17_lowermounts_a_F","polo17_lowermounts_b_F","polo17_shockbottom_F","polo17_lowerarm_F"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //anti-roll
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":""},
         {"selfCollision":false},
         {"collision":true}
         {"nodeWeight":1.7},
         //front anti-roll
         ["arbfr", -0.58, -1.31, 0.25],
         ["arbfl", 0.58, -1.31, 0.25],
         {"group":""},
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        //19mm 1403
        //20mm 1722
        //21mm 2094
        //22mm 2522
        //23mm 3012
        {"spring":2094, "damp":10, "deform":10000, "strength":9999999},
        ["arbfr", "fx2r", "fx2l", "arbfl"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--ANTI-ROLL--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":2501000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":250000},
          //end links
          ["arbfr","fh4r"],
          ["arbfl","fh4l"],
          //rigids
          ["arbfr","fx2r"],
          ["arbfl","fx2l"],
          ["arbfr","fx2l"],
          ["arbfl","fx2r"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_swaybar_F_sport_RS": {
    "information":{
        "authors":"BeamNG",
        "name":"Sport RS Front Sway Bar",
        "value":400,
    },
    "slotType" : "polo17_swaybar_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_swaybar_F", ["polo17_lowermounts_a_F","polo17_lowermounts_b_F","polo17_shockbottom_F","polo17_lowerarm_F"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //anti-roll
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":""},
         {"selfCollision":false},
         {"collision":true}
         {"nodeWeight":1.9},
         //front anti-roll
         ["arbfr", -0.58, -1.31, 0.25],
         ["arbfl", 0.58, -1.31, 0.25],
         {"group":""},
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        //19mm 1403
        //20mm 1722
        //21mm 2094
        //22mm 2522
        //23mm 3012
        {"spring":2522, "damp":10, "deform":10000, "strength":9999999},
        ["arbfr", "fx2r", "fx2l", "arbfl"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--ANTI-ROLL--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":2501000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":250000},
          //end links
          ["arbfr","fh4r"],
          ["arbfl","fh4l"],
          //rigids
          ["arbfr","fx2r"],
          ["arbfl","fx2l"],
          ["arbfr","fx2l"],
          ["arbfl","fx2r"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_swaybar_F_race": {
    "information":{
        "authors":"BeamNG",
        "name":"Race Front Sway Bar",
        "value":650,
    },
    "slotType" : "polo17_swaybar_F",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_swaybar_F", ["polo17_lowermounts_a_F","polo17_lowermounts_b_F","polo17_shockbottom_F","polo17_lowerarm_F"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //anti-roll
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":""},
         {"selfCollision":false},
         {"collision":true}
         {"nodeWeight":2.3},
         //front anti-roll
         ["arbfr", -0.58, -1.31, 0.25],
         ["arbfl", 0.58, -1.31, 0.25],
         {"group":""},
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$arb_spring_F", "range", "N/m", "Suspension", 28000, 5000, 100000, "Anti-Roll Spring Rate", "Stiffness of the anti-roll bar, defined at the end links", {"stepDis":1000,"subCategory":"Front"}]
    ],
    "torsionbars": [
        ["id1:", "id2:", "id3:", "id4:"],
        //motion ratio 1 (difference between real and jbeam sway bar)
        //arm length 0.33
        {"spring":"$=$arb_spring_F*0.33*0.33", "damp":10, "deform":10000, "strength":9999999},
        ["arbfr", "fx2r", "fx2l", "arbfl"],
    ],
    "beams": [
          ["id1:", "id2:"],
          //--ANTI-ROLL--
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":2501000,"beamDamp":100},
          {"beamDeform":15000,"beamStrength":250000},
          //end links
          ["arbfr","fh4r"],
          ["arbfl","fh4l"],
          //rigids
          ["arbfr","fx2r"],
          ["arbfl","fx2l"],
          ["arbfr","fx2l"],
          ["arbfl","fx2r"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_strut_bar": {
    "information":{
        "authors":"BeamNG",
        "name":"Strut Bar",
        "value":200,
    },
    "slotType" : "polo17_strut_bar",
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_strut_bar", ["polo17_strutbar"]],
    ],

    "beams": [
          ["id1:", "id2:"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":3000600,"beamDamp":120},
          {"beamDeform":60000,"beamStrength":500000},
          //rigid beams
          ["fs1l","fs1r"],
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_steering": {
    "information":{
        "authors":"BeamNG",
        "name":"Steering",
        "value":200,
    },
    "slotType" : "polo17_steering",
    "slots": [
        ["type", "default", "description"]
        ["polo17_power_steering","", "Power Steering"],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_tierod_F", ["polo17_tierod_F","polo17_lowermounts_b_F","polo17_steeringbox"]],
    ],
    "rails": {"steeringrack":{"links:":["fh6r", "fh6l"], "broken:":[], "looped":false, "capped":true},
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx5r", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
        ["fx5l", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--steering rod--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_tierod_F"},
         {"nodeWeight":4.75},
         ["fh6r", -0.23, -1.13, 0.285],
         ["fh6l", 0.23, -1.13, 0.285],
         {"group":""},
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$toe_FR", "range", "", "Wheel Alignment", 1.0005, 0.98, 1.02, "Toe Adjust", "Adjusts the wheel toe-in angle", {"subCategory":"Front"}]
        ["$steer_center_F", "range", "", "Wheel Alignment", 0, -0.002, 0.002, "Toe Left/Right Trim", "Fine tunes the centerpoint of the steering", {"subCategory":"Front"}]
    ],
    "beams": [
          ["id1:","id2:"],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":10001000,"beamDamp":150,"beamDeform":79500,"beamStrength":142500},
          ["fh6r","fh6l"],
          //toe out
          {"beamSpring":15001000,"beamDamp":150,"beamDeform":75500,"beamStrength":127500},
          ["fh3r","fh6r", {"beamPrecompression":"$=$toe_FR-$steer_center_F","beamPrecompressionTime":0.5}],
          ["fh3l","fh6l", {"beamPrecompression":"$=$toe_FR+$steer_center_F","beamPrecompressionTime":0.5}],
          //steering damper
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDeform":20000,"beamStrength":35000},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamDamp":80},
          ["fh3r","fx1r", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh3l","fx2l", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5r","fx2r", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5l","fx2l", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "hydros": [
        ["id1:","id2:"],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
        {"beamSpring":10001000,"beamDamp":50,"beamDeform":"FLT_MAX","beamStrength":92500},
        ["fh6r","fx5l", {"factor":-0.22,"steeringWheelLock":510, "inRate":1.25,"outRate":1.25}],
        ["fh6l","fx5r", {"factor":0.22,"steeringWheelLock":510, "inRate":1.25,"outRate":1.25}],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "input": {
        "FFBcoef":"$=$ffbstrength*11",
    },
},
"polo17_steering_race": {
    "information":{
        "authors":"BeamNG",
        "name":"Quick Ratio Race Steering",
        "value":620,
    },
    "slotType" : "polo17_steering",
    "slots": [
        ["type", "default", "description"]
        ["polo17_power_steering","", "Power Steering"],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_tierod_F", ["polo17_tierod_F","polo17_lowermounts_b_F","polo17_steeringbox"]],
    ],
    "rails": {"steeringrack":{"links:":["fh6r", "fh6l"], "broken:":[], "looped":false, "capped":true}
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx5r", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
        ["fx5l", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--steering rod--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_tierod_F"},
         {"nodeWeight":4.75},
         ["fh6r", -0.23, -1.13, 0.285],
         ["fh6l", 0.23, -1.13, 0.285],
         {"group":""},
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$toe_FR", "range", "", "Wheel Alignment", 0.999, 0.98, 1.02, "Toe Adjust", "Adjusts the wheel toe-in angle", {"subCategory":"Front"}]
        ["$steer_center_F", "range", "", "Wheel Alignment", 0, -0.002, 0.002, "Toe Left/Right Trim", "Fine tunes the centerpoint of the steering", {"subCategory":"Front"}]
    ],
    "beams": [
          ["id1:","id2:"],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":10001000,"beamDamp":150,"beamDeform":79500,"beamStrength":142500},
          ["fh6r","fh6l"],
          //toe out
          {"beamSpring":15001000,"beamDamp":150,"beamDeform":75500,"beamStrength":127500},
          ["fh3r","fh6r", {"beamPrecompression":"$=$toe_FR-$steer_center_F","beamPrecompressionTime":0.5}],
          ["fh3l","fh6l", {"beamPrecompression":"$=$toe_FR+$steer_center_F","beamPrecompressionTime":0.5}],
          //steering damper
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDeform":20000,"beamStrength":35000},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamDamp":50},
          ["fh3r","fx1r", {"beamDampVelocitySplit":0.15,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh3l","fx2l", {"beamDampVelocitySplit":0.15,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5r","fx2r", {"beamDampVelocitySplit":0.15,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5l","fx2l", {"beamDampVelocitySplit":0.15,"beamDampFast":800,"dampCutoffHz":750}],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "hydros": [
        ["id1:","id2:"],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
        {"beamSpring":10001000,"beamDamp":50,"beamDeform":"FLT_MAX","beamStrength":92500},
        ["fh6r","fx5l", {"factor":-0.22,"steeringWheelLock":430, "inRate":1.25,"outRate":1.25}],
        ["fh6l","fx5r", {"factor":0.22,"steeringWheelLock":430, "inRate":1.25,"outRate":1.25}],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "input": {
        "FFBcoef":"$=$ffbstrength*11",
    },
},
"polo17_steering_rally": {
    "information":{
        "authors":"BeamNG",
        "name":"Quick Ratio Rally Steering",
        "value":700,
    },
    "slotType" : "polo17_steering",
    "slots": [
        ["type", "default", "description"]
        ["polo17_power_steering","", "Power Steering"],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_tierod_F", ["polo17_tierod_F","polo17_lowermounts_b_F","polo17_steeringbox"]],
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$toe_FR", "range", "", "Wheel Alignment", 0.997, 0.98, 1.02, "Toe Adjust", "Adjusts the wheel toe-in angle", {"subCategory":"Front"}]
        ["$steer_center_F", "range", "", "Wheel Alignment", 0, -0.002, 0.002, "Toe Left/Right Trim", "Fine tunes the centerpoint of the steering", {"subCategory":"Front"}]
    ],
    "rails": {
        "steeringrack":{"links:":["fh6r", "fh6l"], "broken:":[], "looped":false, "capped":true}
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx5r", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
        ["fx5l", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--steering rod--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_tierod_F"},
         {"nodeWeight":4.75},
         ["fh6r", -0.23, -1.13, 0.285],
         ["fh6l", 0.23, -1.13, 0.285],
         {"group":""},
    ],
    "beams": [
          ["id1:","id2:"],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":10001000,"beamDamp":150,"beamDeform":99500,"beamStrength":192500},
          ["fh6r","fh6l"],
          //toe out
          {"beamSpring":15001000,"beamDamp":150,"beamDeform":99500,"beamStrength":192500},
          ["fh3r","fh6r", {"beamPrecompression":"$=$toe_FR-$steer_center_F","beamPrecompressionTime":0.5}],
          ["fh3l","fh6l", {"beamPrecompression":"$=$toe_FR+$steer_center_F","beamPrecompressionTime":0.5}],
          //steering damper
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDeform":20000,"beamStrength":35000},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamDamp":80},
          ["fh3r","fx1r", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh3l","fx2l", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5r","fx2r", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          ["fh5l","fx2l", {"beamDampVelocitySplit":0.1,"beamDampFast":800,"dampCutoffHz":750}],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "hydros": [
        ["id1:","id2:"],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
        {"beamSpring":10001000,"beamDamp":50,"beamDeform":"FLT_MAX","beamStrength":135000},
        ["fh6r","fx5l", {"factor":-0.23,"steeringWheelLock":270, "inRate":1.25,"outRate":1.25}],
        ["fh6l","fx5r", {"factor":0.23,"steeringWheelLock":270, "inRate":1.25,"outRate":1.25}],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "input": {
        "FFBcoef":"$=$ffbstrength*10",
    },
},
"polo17_steering_drift": {
    "information":{
        "authors":"BeamNG",
        "name":"Quick Ratio Drift Steering",
        "value":700,
    },
    "slotType" : "polo17_steering",
    "slots": [
        ["type", "default", "description"]
        ["polo17_power_steering","", "Power Steering"],
    ],
    "flexbodies": [
        ["mesh", "[group]:", "nonFlexMaterials"],
        ["polo17_tierod_F", ["polo17_tierod_F","polo17_lowermounts_a_F","polo17_steeringbox"]],
    ],
    "rails": {"steeringrack":{"links:":["fh6r", "fh6l"], "broken:":[], "looped":false, "capped":true}
    },
    "slidenodes": [
        ["id:", "railName", "attached", "fixToRail", "tolerance", "spring", "strength", "capStrength"],
        ["fx5r", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
        ["fx5l", "steeringrack", true, true, 0.0, 15001000, "FLT_MAX", "FLT_MAX"],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--steering rod--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_tierod_F"},
         {"nodeWeight":4.75},
         ["fh6r", -0.25, -1.13, 0.285],
         ["fh6l", 0.25, -1.13, 0.285],
         //tie rod end -- overwritten with drift steering
         {"nodeWeight":5.0},
         ["fh3r",-0.68, -1.165, 0.26, {"group":["polo17_tierod_F","polo17_hub_F"]}],
         ["fh3l", 0.68, -1.165, 0.26, {"group":["polo17_tierod_F","polo17_hub_F"]}],
         {"group":""},
    ],
    "variables": [
        ["name", "type", "unit", "category", "default", "min", "max", "title", "description"]
        ["$toe_FR", "range", "", "Wheel Alignment", 1.0, 0.98, 1.02, "Toe Adjust", "Adjusts the wheel toe-in angle", {"subCategory":"Front"}]
        ["$steer_center_F", "range", "", "Wheel Alignment", 0, -0.002, 0.002, "Toe Left/Right Trim", "Fine tunes the centerpoint of the steering", {"subCategory":"Front"}]
    ],
    "beams": [
          ["id1:","id2:"],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
          {"beamSpring":10001000,"beamDamp":150,"beamDeform":79500,"beamStrength":142500},
          ["fh6r","fh6l"],
          //toe out
          {"beamSpring":15001000,"beamDamp":150,"beamDeform":79500,"beamStrength":142500},
          ["fh3r","fh6r", {"beamPrecompression":"$=$toe_FR-$steer_center_F","beamPrecompressionTime":0.5}],
          ["fh3l","fh6l", {"beamPrecompression":"$=$toe_FR+$steer_center_F","beamPrecompressionTime":0.5}],
          //steering damper
          {"beamPrecompression":1.0, "beamType":"|BOUNDED", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":0,"beamDeform":20000,"beamStrength":35000},
          {"beamLimitSpring":0,"beamLimitDamp":0},
          {"beamDamp":80},
          ["fh3r","fx1r", {"beamDampVelocitySplit":0.2,"beamDampFast":1600,"dampCutoffHz":750}],
          ["fh3l","fx2l", {"beamDampVelocitySplit":0.2,"beamDampFast":1600,"dampCutoffHz":750}],
          ["fh5r","fx2r", {"beamDampVelocitySplit":0.2,"beamDampFast":1600,"dampCutoffHz":750}],
          ["fh5l","fx2l", {"beamDampVelocitySplit":0.2,"beamDampFast":1600,"dampCutoffHz":750}],
          {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "hydros": [
        ["id1:","id2:"],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
        {"beamSpring":10001000,"beamDamp":50,"beamDeform":"FLT_MAX","beamStrength":92500},
        ["fh6r","fx5l", {"factor":-0.29,"steeringWheelLock":450, "inRate":1.25,"outRate":1.25}],
        ["fh6l","fx5r", {"factor":0.29,"steeringWheelLock":450, "inRate":1.25,"outRate":1.25}],
        {"beamPrecompression":1.0, "beamType":"|NORMAL", "beamLongBound":1, "beamShortBound":1},
    ],
    "input": {
        "FFBcoef":"$=$ffbstrength*12",
    },
},
"polo17_power_steering": {
    "information":{
        "authors":"BeamNG",
        "name":"Power Steering",
        "value":250,
    }
    "slotType" : "polo17_power_steering",
    "controller": [
        ["fileName"],
        ["powerSteering", {"strengthFast":1, "strengthSlow": 0.10, "speedSlow": 2, "speedFast": 20, "constantOffset":-0.05}],
    ],
},
}