{
"polo17_engine_1.0_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 1.0L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
        ["polo17_intake2","", "Turbo"],
		["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],       
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500,  35],
            [1000,  48],
            [2000,  65],
            [3000,  80],
            [4000,  93],
            [5000, 100],
            [6000, 105],
            [7000, 100],
            [8000,  93],
            [9000,  70],
            [10000, 48],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.05,
        "friction":10,
        "dynamicFriction":0.025,
        "engineBrakeTorque":20,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 430,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
    "soundConfig": {
        "sampleName": "i3_2_engine",
        "intakeMuffling": 1,

        "mainGain": -14,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.7,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.1,

        "eqHighGain": -7,
        "eqHighFreq": 4500,
        "eqHighWidth": 0.1

        "lowShelfGain":3,
        "lowShelfFreq":120,

        "highShelfGain":0,
        "highShelfFreq":2500,

        "fundamentalFrequencyCylinderCount":3,
        "eqFundamentalGain":0,
    },
    "soundConfigExhaust": {
        "sampleName": "i3_2_exhaust",

        "mainGain": -4,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.8,
        "minLoadMix": 0,

        "eqLowGain": 4,
        "eqLowFreq": 450,
        "eqLowWidth": 0.25,

        "eqHighGain": 0,
        "eqHighFreq": 400,
        "eqHighWidth": 0.1,

        "lowShelfGain":-5,
        "lowShelfFreq":80,

        "highShelfGain":6,
        "highShelfFreq":2500,

        "fundamentalFrequencyCylinderCount":3,
        "eqFundamentalGain": -4,
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":11},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_1.2_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 1.2L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
        ["polo17_intake2","", "Turbo"],
		["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],    
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 42],
            [1000, 57],
            [2000, 78],
            [3000, 96],
            [4000, 111],
            [5000, 120],
            [6000, 126],
            [7000, 120],
            [8000, 111],
            [9000, 84],
            [10000, 57],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.06,
        "friction":12,
        "dynamicFriction":0.025,
        "engineBrakeTorque":24,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 400,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
    "soundConfig": {
        "sampleName": "i3_2_engine",
        "intakeMuffling": 1,

        "mainGain": -14,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.7,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.1,

        "eqHighGain": -7,
        "eqHighFreq": 4500,
        "eqHighWidth": 0.1

        "lowShelfGain":3,
        "lowShelfFreq":120,

        "highShelfGain":0,
        "highShelfFreq":2500,

        "fundamentalFrequencyCylinderCount":3,
        "eqFundamentalGain":0,
    },
    "soundConfigExhaust": {
        "sampleName": "i3_2_exhaust",

        "mainGain": -4,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.8,
        "minLoadMix": 0,

        "eqLowGain": 4,
        "eqLowFreq": 450,
        "eqLowWidth": 0.25,

        "eqHighGain": 0,
        "eqHighFreq": 400,
        "eqHighWidth": 0.1,

        "lowShelfGain":-5,
        "lowShelfFreq":80,

        "highShelfGain":6,
        "highShelfFreq":2500,

        "fundamentalFrequencyCylinderCount":3,
        "eqFundamentalGain": -4,
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":12},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_1.4_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 1.4L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
       ["polo17_intake2","", "Turbo"],
	   ["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],       
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500,   49],
            [1000,  67],
            [2000,  91],
            [3000, 112],
            [4000, 130],
            [5000, 140],
            [6000, 147],
            [7000, 140],
            [8000, 130],
            [9000,  98],
            [10000, 67],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.07,
        "friction":14,
        "dynamicFriction":0.025,
        "engineBrakeTorque":28,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 560,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
   "soundConfig": {
        "sampleName": "I4_3_engine",
        "intakeMuffling": 1,

        "mainGain": -13,
        "onLoadGain":1,
        "offLoadGain":0.45,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.1,

        "eqHighGain": 0,
        "eqHighFreq": 500,
        "eqHighWidth": 0.1,

        "lowShelfGain":2,
        "lowShelfFreq":150,

        "highShelfGain":4,
        "highShelfFreq":7500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain":0,
    },
    "soundConfigExhaust": {
        "sampleName": "I4_3_exhaust",

        "mainGain": -2,
        "onLoadGain":1,
        "offLoadGain":0.58,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.2,

        "eqHighGain": 0,
        "eqHighFreq": 4000,
        "eqHighWidth": 0.1,

        "lowShelfGain":3,
        "lowShelfFreq":120,

        "highShelfGain":4,
        "highShelfFreq":6500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain": -3
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":13},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_1.6_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 1.6L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
        ["polo17_intake2","", "Turbo"],
		["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],         
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 56],
            [1000, 76],
            [2000, 104],
            [3000, 128],
            [4000, 148],
            [5000, 160],
            [6000, 168],
            [7000, 160],
            [8000, 148],
            [9000, 112],
            [10000, 76],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.08,
        "friction":16,
        "dynamicFriction":0.025,
        "engineBrakeTorque":32,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 640,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
   "soundConfig": {
        "sampleName": "I4_3_engine",
        "intakeMuffling": 1,

        "mainGain": -13,
        "onLoadGain":1,
        "offLoadGain":0.45,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.1,

        "eqHighGain": 0,
        "eqHighFreq": 500,
        "eqHighWidth": 0.1,

        "lowShelfGain":2,
        "lowShelfFreq":150,

        "highShelfGain":4,
        "highShelfFreq":7500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain":0,
    },
    "soundConfigExhaust": {
        "sampleName": "I4_3_exhaust",

        "mainGain": -2,
        "onLoadGain":1,
        "offLoadGain":0.58,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.2,

        "eqHighGain": 0,
        "eqHighFreq": 4000,
        "eqHighWidth": 0.1,

        "lowShelfGain":3,
        "lowShelfFreq":120,

        "highShelfGain":4,
        "highShelfFreq":6500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain": -3
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":14},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_1.8_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 1.8L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
       ["polo17_intake2","", "Turbo"],
	   ["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],       
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 63],
            [1000, 86],
            [2000, 117],
            [3000, 144],
            [4000, 167],
            [5000, 180],
            [6000, 189],
            [7000, 180],
            [8000, 167],
            [9000, 126],
            [10000, 86],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.09,
        "friction":18,
        "dynamicFriction":0.025,
        "engineBrakeTorque":36,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 720,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
   "soundConfig": {
        "sampleName": "I4_3_engine",
        "intakeMuffling": 1,

        "mainGain": -13,
        "onLoadGain":1,
        "offLoadGain":0.45,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.1,

        "eqHighGain": 0,
        "eqHighFreq": 500,
        "eqHighWidth": 0.1,

        "lowShelfGain":2,
        "lowShelfFreq":150,

        "highShelfGain":4,
        "highShelfFreq":7500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain":0,
    },
    "soundConfigExhaust": {
        "sampleName": "I4_3_exhaust",

        "mainGain": -2,
        "onLoadGain":1,
        "offLoadGain":0.58,

        "maxLoadMix": 0.67,
        "minLoadMix": 0,

        "eqLowGain": 0,
        "eqLowFreq": 120,
        "eqLowWidth": 0.2,

        "eqHighGain": 0,
        "eqHighFreq": 4000,
        "eqHighWidth": 0.1,

        "lowShelfGain":3,
        "lowShelfFreq":120,

        "highShelfGain":4,
        "highShelfFreq":6500,

        "fundamentalFrequencyCylinderCount":4,
        "eqFundamentalGain": -3
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":15},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_2.0_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 2.0L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
       ["polo17_intake2","", "Turbo"],
	   ["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],         
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 70],
            [1000, 95],
            [2000, 130],
            [3000, 160],
            [4000, 185],
            [5000, 200],
            [6000, 210],
            [7000, 200],
            [8000, 185],
            [9000, 140],
            [10000, 95],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.1,
        "friction":20,
        "dynamicFriction":0.025,
        "engineBrakeTorque":40,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 800,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
    "soundConfig": {
        "sampleName": "i5_engine",
        "intakeMuffling": 1,

        "mainGain": -13,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.75,
        "minLoadMix": 0,

        "eqLowGain": 5,
        "eqLowFreq": 500,
        "eqLowWidth": 0.2,

        "eqHighGain": 0,
        "eqHighFreq": 1000,
        "eqHighWidth": 0.1,

        "lowShelfGain":0,
        "lowShelfFreq":80,

        "highShelfGain":8,
        "highShelfFreq":2500,

        "fundamentalFrequencyCylinderCount":5,
        "eqFundamentalGain":5,
    },
    "soundConfigExhaust": {
        "sampleName": "i5_exhaust",

        "mainGain": 1,
        "onLoadGain":1,
        "offLoadGain":0.52,

        "maxLoadMix": 0.75,
        "minLoadMix": 0,

        "eqLowGain": 7,
        "eqLowFreq": 450,
        "eqLowWidth": 0.2,

        "eqHighGain": 7,
        "eqHighFreq": 1400,
        "eqHighWidth": 0.1,

        "lowShelfGain":-5,
        "lowShelfFreq":90,

        "highShelfGain":10,
        "highShelfFreq":4000,

        "fundamentalFrequencyCylinderCount":5,
        "eqFundamentalGain": -3,
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":16},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_2.2_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 2.2L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
       ["polo17_intake2","", "Turbo"],
	   ["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],         
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 77],
            [1000, 105],
            [2000, 143],
            [3000, 176],
            [4000, 204],
            [5000, 220],
            [6000, 231],
            [7000, 220],
            [8000, 204],
            [9000, 154],
            [10000, 105],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.11,
        "friction":22,
        "dynamicFriction":0.025,
        "engineBrakeTorque":44,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 880,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
   "soundConfig": {
        "sampleName": "I6_2_engine",
        "intakeMuffling": 1,
        "mainGain": -10,
        "onLoadGain":1,
        "offLoadGain":0.53,
        "maxLoadMix": 0.7,
        "minLoadMix": 0,
        "eqLowGain": 6,
        "eqLowFreq": 250,
        "eqLowWidth": 0.3,
        "eqHighGain": -10,
        "eqHighFreq": 1500,
        "eqHighWidth": 0.15,
        "lowShelfGain":-1,
        "lowShelfFreq":150,
        "highShelfGain":2,
        "highShelfFreq":6000,
        "fundamentalFrequencyCylinderCount":6,
        "eqFundamentalGain": -5,
    },
    "soundConfigExhaust": {
        "sampleName": "I6_2_exhaust",
        "mainGain": 3,
        "onLoadGain":1,
        "offLoadGain":0.40,
        "maxLoadMix": 0.7,
        "minLoadMix": 0,
        "eqLowGain": -6,
        "eqLowFreq": 1200,
        "eqLowWidth": 0.2,
        "eqHighGain": -3,
        "eqHighFreq": 3000,
        "eqHighWidth": 0.2,
        "lowShelfGain":6,
        "lowShelfFreq":450,
        "highShelfGain":-14,
        "highShelfFreq":5500,
        "fundamentalFrequencyCylinderCount":6,
        "eqFundamentalGain": -4,
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":17},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
"polo17_engine_2.4_B": {
    "information":{
        "authors":"BeamNG",
        "name":"B 2.4L I4 Engine",
        "value":3800,
    },
    "slotType" : "polo17_engine",
    "slots": [
        ["type", "default", "description"],
        ["polo17_exhaust_I4","polo17_exhaust_I4", "Exhaust"],
        ["polo17_enginemounts","polo17_enginemounts", "Engine Mounts", {"coreSlot":true}],
       ["polo17_intake2","", "Turbo"],
	   ["polo17_block_B","stock_engine_block_B", "Engine Long Block", {"coreSlot":true}],
        ["polo17_oilpan","polo17_oilpan", "Oil Pan", {"coreSlot":true}],         
        ["polo17_transmission","polo17_transmission", "Transmission"],
    ],
    "powertrain": [
        ["type", "name", "inputName", "inputIndex"],
        ["combustionEngine", "mainEngine", "dummy", 0],
    ],
    "mainEngine":{
        "torque":[
            ["rpm", "torque"],
            [0, 0],
            [500, 84],
            [1000, 114],
            [2000, 156],
            [3000, 192],
            [4000, 222],
            [5000, 240],
            [6000, 252],
            [7000, 240],
            [8000, 222],
            [9000, 168],
            [10000, 114],
        ],

        "idleRPM":950,
        //max rpm physically capable of
        "maxRPM":6500,
        "inertia":0.12,
        "friction":24,
        "dynamicFriction":0.025,
        "engineBrakeTorque":48,     
        "burnEfficiency":[
			[0, 0.12],
			[0.05, 0.30],
			[0.4, 0.48],
			[0.7, 0.50],
			[1, 0.37],
        ],
        //fuel system
        "energyStorage": "mainTank",
        "requiredEnergyType":"gasoline",

        //exhaust
        "instantAfterFireSound": "event:>Vehicle>Afterfire>i4_01>single",
        "sustainedAfterFireSound": "event:>Vehicle>Afterfire>i4_01>multi",
        "shiftAfterFireSound": "event:>Vehicle>Afterfire>i4_01>shift",
        "particulates":0.015,
        "instantAfterFireCoef": 0.75,
        "sustainedAfterFireCoef": 0.75,
        "instantAfterFireVolumeCoef": 1.0,
        "sustainedAfterFireVolumeCoef": 0.6,
        "shiftAfterFireVolumeCoef": 0.75,
		
        //cooling and oil system
        "thermalsEnabled":true,
        "engineBlockMaterial":"aluminum",
        "oilVolume":4,
		
        //engine durability
        "cylinderWallTemperatureDamageThreshold":130,
        "headGasketDamageThreshold":1500000,
        "pistonRingDamageThreshold":1500000,
        "connectingRodDamageThreshold":2000000,
        "maxTorqueRating": 960,
        "maxOverTorqueDamage": 350,

        //node beam interface
        "torqueReactionNodes:":["e1l","e2l","e4r"],
        "waterDamage": {"[engineGroup]:":["engine_intake"]},
        "radiator": {"[engineGroup]:":["radiator"]},
        "engineBlock": {"[engineGroup]:":["engine_block"]},
        "breakTriggerBeam":"engine",
        "uiName":"Engine",
        "soundConfig": "soundConfig",
        "soundConfigExhaust": "soundConfigExhaust",

        //starter motor
        "starterSample":"event:>Engine>Starter>i4_2001_eng",
        "starterSampleExhaust":"event:>Engine>Starter>i4_2001_exh",
        "shutOffSampleEngine":"event:>Engine>Shutoff>i4_2001_eng",
        "shutOffSampleExhaust":"event:>Engine>Shutoff>i4_2001_exh",
        "starterVolume":0.62,
        "starterVolumeExhaust":0.6,
        "shutOffVolumeEngine":0.3,
        "shutOffVolumeExhaust":0.36,
        "starterThrottleKillTime":0.6,
        "idleRPMStartRate":2,
        "idleRPMStartCoef":1,

        //damage deformGroups
        "deformGroups":["mainEngine", "mainEngine_piping", "mainEngine_accessories"]
        "deformGroups_oilPan":["oilpan_damage"]
    },
   "soundConfig": {
        "sampleName": "I6_2_engine",
        "intakeMuffling": 1,
        "mainGain": -10,
        "onLoadGain":1,
        "offLoadGain":0.53,
        "maxLoadMix": 0.7,
        "minLoadMix": 0,
        "eqLowGain": 6,
        "eqLowFreq": 250,
        "eqLowWidth": 0.3,
        "eqHighGain": -10,
        "eqHighFreq": 1500,
        "eqHighWidth": 0.15,
        "lowShelfGain":-1,
        "lowShelfFreq":150,
        "highShelfGain":2,
        "highShelfFreq":6000,
        "fundamentalFrequencyCylinderCount":6,
        "eqFundamentalGain": -5,
    },
    "soundConfigExhaust": {
        "sampleName": "I6_2_exhaust",
        "mainGain": 3,
        "onLoadGain":1,
        "offLoadGain":0.40,
        "maxLoadMix": 0.7,
        "minLoadMix": 0,
        "eqLowGain": -6,
        "eqLowFreq": 1200,
        "eqLowWidth": 0.2,
        "eqHighGain": -3,
        "eqHighFreq": 3000,
        "eqHighWidth": 0.2,
        "lowShelfGain":6,
        "lowShelfFreq":450,
        "highShelfGain":-14,
        "highShelfFreq":5500,
        "fundamentalFrequencyCylinderCount":6,
        "eqFundamentalGain": -4,
    },
    "vehicleController": {
        "clutchLaunchStartRPM":2000,
        "clutchLaunchTargetRPM":2800,
        //**highShiftDown can be overwritten by automatic transmissions**
        "highShiftDownRPM":4800 //[0,0,0,3800,4400,4600,4800,4800]
        //**highShiftUp can be overwritten by intake modifications**
        "highShiftUpRPM":6400,
    },
    "flexbodies": [
         ["mesh", "[group]:", "nonFlexMaterials"],
         ["polo17_engine", ["polo17_engine","polo17_transmission"]],
         ["polo17_intake_NA", ["polo17_engine","polo17_transmission"]],
         ["polo17_engbaycrap", ["polo17_body"]],
    ],
    "nodes": [
         ["id", "posX", "posY", "posZ"],
         //--2.0L I4 Engine--
         {"selfCollision":false},
         {"collision":true},
         {"nodeMaterial":"|NM_METAL"},
         {"frictionCoef":0.5},
         {"group":"polo17_engine"},
         {"engineGroup":"engine_block"},
         {"nodeWeight":18},
         ["e1r", -0.34, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e1l", -0.34, -1.26, 0.36],
         ["e2r", 0.17, -1.57, 0.36,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e2l", 0.17, -1.26, 0.36],
         {"engineGroup":["engine_block","engine_intake"]},
         ["e3r", -0.34, -1.57, 0.77,{"chemEnergy":1000,"burnRate":0.39,"flashPoint":1000,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e3l", -0.34, -1.26, 0.77],
         ["e4r", 0.17, -1.57, 0.77,{"isExhaust":"mainEngine","chemEnergy":1000,"burnRate":0.39,"flashPoint":800,"specHeat": 0.2,"selfIgnitionCoef":false,"smokePoint":900,"baseTemp":"thermals","conductionRadius":0.15}],
         ["e4l", 0.17, -1.26, 0.77],
         {"engineGroup":""},
         {"group":""},
         //engine mount nodes
         ["em1r", -0.42, -1.4, 0.7, {"nodeWeight":3}],
         ["em2l", 0.27, -1.4, 0.55, {"nodeWeight":3}],
    ],
    "beams": [
          ["id1:", "id2:"],
          {"beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
          {"beamSpring":15001000,"beamDamp":500},
          {"beamDeform":250000,"beamStrength":"FLT_MAX"},
          //engine
          {"deformGroup":"mainEngine", "deformationTriggerRatio":0.001}
          ["e1r","e1l"],
          ["e2r","e2l"],
          ["e3r","e3l"],
          ["e4r","e4l"],
          ["e1r","e2r"],
          ["e1l","e2l"],
          ["e3r","e4r"],
          ["e3l","e4l"],
          ["e1r","e3r"],
          ["e1l","e3l"],
          ["e2r","e4r", {"isExhaust":"mainEngine"}],
          ["e2l","e4l"],
          ["e2r","e3r"],
          ["e2l","e3l"],
          ["e2r","e3l"],
          ["e2l","e3r"],
          ["e1r","e4r"],
          ["e1l","e4l"],
          ["e1r","e4l"],
          ["e1l","e4r"],
          ["e1r","e2l"],
          ["e1l","e2r"],
          ["e3r","e4l"],
          ["e3l","e4r"],
          ["e1r","e3l"],
          ["e1l","e3r"],
          ["e2r","e4l"],
          ["e2l","e4r"],
          //engine mount nodes
          {"beamSpring":3400000,"beamDamp":150},
          {"beamDeform":90000,"beamStrength":"FLT_MAX"},
          ["em1r","e3l"],
          ["em1r","e3r"],
          ["em1r","e4l"],
          ["em1r","e4r"],
          ["em1r", "e1r"],
          ["em1r", "e1l"],
          ["em1r", "e2l"],
          ["em1r", "e2r"],
          ["em2l","e3l"],
          ["em2l","e3r"],
          ["em2l","e4l"],
          ["em2l","e4r"],
          ["em2l", "e1r"],
          ["em2l", "e1l"],
          ["em2l", "e2l"],
          ["em2l", "e2r"],
          {"deformGroup":""},
          {"beamPrecompression":1, "beamType":"|NORMAL", "beamLongBound":1.0, "beamShortBound":1.0},
    ],
},
}